Control Module Template

Drill four 1/4"ich holes

Please cut this template on the outside lines and tape to the left inner fender.

Ensure there is no interference with the hood hinge when closing.

 Drill two holes 5/16 inch, install the control module with the wires exiting from the bottom of the module or if you would like to install the module horizontal and have your wires exiting to the front of the car.